Station: 						Tycor Waterworks
County:							Waterford
Met Éireann Reference Code:				RR/D/3/26
Lat:							52°15'10"N [approx.]
Lon:							07°07'50"W [approx.]
Observer:						Records completed by M.J. Fleming; O'Rourke; Sheedy
Start year:						1888
End year:						1939
Missing:						1889; 1926; 1st Feb-6th Apr 1928; 1932-1937
Missing data indicator:					-999
Time of Observation:					09:00am
Unit of measurement:					inch				
Rain gauge pattern:					n/a
Gauge diameter:						5 inches			
Height of top of gauge above ground:			7 inches
Height of top of gauge above sea level:			170 feet
Nearest railway station:				Tramore
Distance to nearest railway station:			7 miles South

Additional Information:					1925: Multiday accumulations 20th-31st May; 1st-30th Jun; 1st-13th Jul.
							1927: 1928: Observer notes suggest record is too low. 
							1928: 1st Feb-6th Apr missing.
 

Notes:							1925: May 20th-1st July estimated by surrounding stations.
							1927: Letter to observer about 4 inches low. Ref file 662568/26
							1928: Gauge out of order in 1st Feb to 6th Apr. 
							1928: Record is much too low.
							1930: Bad since 1925. Far too low. Year about 20 inches. 

Rainfall quality indicator:				0: Ok
							1: estimated
							2: daily value not available, accumulated value later
							3: Estimated and Cumulative (read)
							4: Trace (<0.05mm, entered as 0.0)
							5: Estimated Trace (same as 4)
							6: Cumulative Trace (same as 4)
							7: Estimated Cumulative Trace (same as 4)
							8: Not Available (no value entered)
							9: Cumulative value including preceding days with indicator 2 (read)

